MTRN4230

Assignment 4

Runkai Zhao, z5146927

(Notice: The MATLAB programming of question 1, 2, and 4 has been uploaded as following of this report on Microsoft Team.)

# Question 1

## Specify a joint space trajectory formed by quintic polynomials using the ‘jtraj’ function and a period of 3 seconds between q1 and q2.

## A close up of a map Description automatically generated

## Specify a joint space trajectory formed by lspb velocity profiles using the ‘mtraj’ function and a period of 3 seconds between q1 and q2

* 1. A close up of a map

     Description automatically generated

## Specify a straight-line trajectory using the ‘ctraj’ function and a period of 3 seconds between q1 and q2

A close up of a map

Description automatically generated

## Discuss the difference in performance between the three trajectories above in terms of the joint angles, velocities, accelerations, and jerks

* 1. Answer:

“jtraj” computing a joint space trajectory is to utilize the quintic polynomial for calculating the values of velocities and accelerations, so the graphs produced by this method is relatively smoothy and continuous. “mtraj” multi-segment multi-axis trajectory applies the scalar trajectory function, “lspb” option, for a trapezoidal trajectory, which includes linear motion and polynomial blends. It is clear that the plots of velocity, acceleration and jerk are discontinuous, but the overall trends of the function plots over time is much similar to graphs produced by “jtraj”. Both two methods could build an arc trajectory between two given points, and the locus plots of end effector are same. “ctraj” could generate Cartesian trajectory of a straight line between two poses. The velocities of two joints are decreased over time, rather than first increase then decrease, so the acceleration and jerk are also different from “jtraj” and “mtraj”. Obviously, the locus of end effector is a linear line.

# Question 2

## Plot the obstacles above and below the robot arm

* 1. A screenshot of a cell phone

     Description automatically generatedA picture containing stationary

     Description automatically generated

## Generate the shortest path using D\* and plot it in the discrete joint space overlaid on the cost map.

A close up of a logo

Description automatically generated

A screenshot of a cell phone

Description automatically generated

## Convert this path back to joint angles and animate the robot to follow the path

![A screenshot of a cell phone

Description automatically generated]()

## Generate a path using PRM and plot it in the discrete joint space overlaid on the road map.

A close up of a logo

Description automatically generated

A screenshot of a cell phone

Description automatically generated

## Convert this path back to joint angles and animate the robot to follow the path

![A screenshot of a cell phone

Description automatically generated]()

## Describe and discuss the difference between the paths generated in terms of the algorithms used

These two algorithms can produce feasible trajectories from the start point to the target point without violating the motion boundaries. Compared with the PRM algorithm, it can be seen that the D\* algorithm could generate more dense and continuous cell points of joint space on the map, which leads the animation of the robot movement smoothy.

# Question 3

## Two-link manipulator with the below Jacobian, what are the torques at the joints needed to apply a force vector °F = 10 X0?

# Question 4

## Inertia Matrix

## D Matrix (Acceleration-related inertia matrix term)

A screenshot of a cell phone screen with text

Description automatically generatedA close up of text on a white background

Description automatically generated![A screenshot of a cell phone

Description automatically generated]()

## C matrix

![A screenshot of a cell phone

Description automatically generated]()

## Kinetic Energy

A screenshot of a cell phone

Description automatically generated

## Potential Energy

A picture containing knife

Description automatically generated

## g Matrix

![A screenshot of a cell phone

Description automatically generated]()